**The effect of Bed Thickness on Hillslope Geometry in Last Chance Canyon, New Mexico**

Sam Anderson1, Nicole Gasparini1, Joel Johnson2, Grace Guryan2, Sophia Brieler1, Mikey Sison2

1Earth and Environmental Science, Tulane University, New Orleans, 70118, USA

2Jackson School of Geosciences, University of Texas at Austin, Austin, 78712, USA

*Correspondence to*: Sam Anderson ([sanderson@tulane.edu](mailto:sanderson@tulane.edu))

*This study challenges conventional paradigms of arid bedrock landscapes, enriching our understanding of geological processes and their role in landscape evolution. Hillslopes in Last Chance Canyon, New Mexico, adopt a convex diffusive shape above an adjusting section of the landscape despite limited regolith, a unique departure from traditional expectations. We propose that variations in bedrock bed thickness significantly influence hillslope configuration and enable relict and low sloping parts of the landscape to exist despite base level fall. Thinner bedrock fosters a diffusive geometry akin to the idealized convex hillslopes found in soil-mantled landscapes, and thicker bedrock inhibits erosional signal propagating upslope due to baselevel fall. Leveraging high-resolution drone imagery, we constructed orthomosaics and digital surface models (DSMs) for seven hillslope transects in two headwater catchments. Our measurements of bed thicknesses, slope, and curvature demonstrate the control that bedrock properties and uplift have on hillslope geometry. Of notable significance is the role of large beds in engendering inflection points across the landscape. These inflection points enable or blur the signal base level fall has on landscape morphology, depending on bed competency and proximity to the erosional signal originating at the base of the mountains.*

The field of geomorphology has long been driven by a quest to understand the temporal evolution of landscapes. Within this context, the concept of "space-for-time substitution" has proven to be a valuable tool, allowing researchers to investigate how landscapes change and mature over time (Schoenbohm et al., 2004; Gallen et al., 2011; Anderson et al., 2012; Prince and Spotila, 2013). This approach involves discerning transitions between low and high relief surfaces, identifying boundaries between areas of differing erosion rates (Mudd and Furbish, 2007; Hurst et al., 2012). Understanding the geomorphic evolution of landscapes is essential for deciphering the history and development of landforms. Researchers have often employed this "space-for-time substitution" to explore how landscapes change and mature over time. This method relies on the spatial progression of landforms, a pattern that transitions from "young to old" under specific environmental conditions. Here we investigate the interplay between relevant bedrock properties, topographic change, and the evolution of Last Chance Canyon in southern New Mexico. We use the space for time argument to describe how an erosional wave formed as a result of base level fall is attenuated by thick beds as it propagates upslope, leaving a unique signal etched into the landscape.

While previous studies have explored landscape transience driven by knickpoints upstream within the channel network, our work introduces a novel perspective by considering the influence of large exposed beds rather than the nature of the underlying bedrock (Mudd and Furbish, 2007; Hurst et al., 2012). We contend that these substantial beds protect the landscape above them from upslope moving erosional wave, causing the landscape to appear diffuse and shallow above large enough beds. Our measurements, facilitated by high-resolution drone imagery, provide a visual narrative of the landscape's temporal transformation, offering insights into the broader implications of these findings for our understanding of geomorphic processes and landscape evolution. Our research raises several key questions and challenges prior work in this territory. We seek to elucidate the impact of bed thickness variations on hillslope geometry, the influence of hillslope location- relative to the erosional signal originating at the base of the range- and elevation its form, and the combined effects of these variables on the landscape's morphology.

Here, we explore landscape transience across multiple hillslopes and in different sections of the same hillslope. Our primary focus is on the concept of "ideality" in hillslope morphology, where specific points on the landscape appear to exhibit idealized states used to describe the form of soil mantled landscapes. We propose that, in bedrock landscapes, these ideal conditions exist due to interplay between bedrock properties and the historical context of the landscape. Here, we challenge conventional paradigms in the field of geomorphology by demonstrating that the presence of thick or thin beds, rather than the nature of the underlying bedrock, significantly influences the "ideality" of the landscape. Furthermore, we demonstrate that “ideal” landscapes can exist in arid bedrock landscapes and demonstrate the mechanisms that generate conditions necessary for these diffuse relict landscapes to propagate temporally.

Throughout this research, we draw upon previous studies that have explored landscape transience and the influence of erosion rates on hillslopes (Schoenbohm et al., 2004; Gallen et al., 2011; Anderson et al., 2012; Prince and Spotila, 2013). We aim to discern whether Last Chance Canyon exhibits patterns of hillslope disturbance, as observed in other landscapes where intensified erosion occurs downstream of channel knickpoints (Mudd and Furbish, 2007; Hurst et al., 2012). Additionally, we consider how perturbations propagate upstream and affect the entire landscape, driven by factors such as drainage area and sediment transport (Whipple and Tucker, 1999; Royden and Perron, 2013; Mudd and Furbish, 2007; Reinhardt et al., 2007; Prince and Spotila, 2013). By investigating the interplay between ridgetop curvature and hillslope relief, we aim to identify indicators of landscape transience, building upon previous studies by Roering et al. (2007) and Hurst et al. (2013a). In summary, our research sets out to advance the field of geomorphology by exploring the role of large beds in landscape evolution, challenging existing paradigms, and enhancing our understanding of geomorphic processes. Through a comprehensive analysis of Last Chance Canyon, we strive to uncover the complexities that govern landform development and contribute to the broader knowledge of landscape dynamics.



**Figure 2 - a. Slope map of Last Chance canyon with values plotted across it. The contour lines correspond to elevations which are interpreted as approximate inflection points for hill and channel slope (1550m for LC 3 and 1640m for LC 1). b. Percentage of slope values from the hillslopes in LC3 and LC1. c. Cumulative frequency plots of bed thicknesses from the 4 surveyed hillslope transects on LC3 and the 3 surveyed hillslope transects on LC1. CHANGE OUTLINE OF LC3 SAME AS SLOPE VALUE**

The research presented here is from two proximal low order watersheds, called LC1 and LC3 in Last Chance Canyon, southern New Mexico, USA. We sampled 3 transects in LC1 and 4 transects in LC3 to capture variations in bed thickness and hillslope morphology. Last Chance Canyon has horizontally bedded to near-horizontal bedrock, and it is currently tectonically inactive (Hill, 1987; Hill, 2006). Last Chance Canyon's geological characteristics have been shaped by its Permian-era origins, with interbedded carbonate and siliciclastic bedrock of varying thicknesses deposited in a shallow lagoon behind a reef complex to the south (Hill, 2000; Phelps et al., 2008; Kerans et al., 2017). The Guadalupe Mountains experienced uplift during basin and range extension approximately 27 million years ago, exposing previously buried bedrock, (Chapin and Cather, 1994; Ricketts et al., 2014; Hoffman, 2014; Decker et al. 2018). LC3 and LC1 differ notably in terms of elevation and slope. LC1, at a slightly higher elevation, features generally lower slopes, while LC3 displays somewhat steeper slopes. Bed thickness comparisons show similarities between LC1 and LC3, but notably thicker beds are evident in the downstream-most transect of LC3.

In March and May 2018, and in February 2021, we measured depth to saprolite and bedrock in the seven transects (3 in LC1 and 4 in LC3), aligning our measurements with ≈12.2 m contour intervals from USGS topographic contour maps to ensure convenient and unbiased sampling. Both LC1 and LC3 display minimal regolith, with an average depth to saprolite of 5.6 cm and depth to bedrock of 20.1 cm. We used a drone to take photos of the 7 hillslope transects at approximately 20 meters above the highest elevation of the 7 hillslope transects and used Agisoft photoscan to generate high resolution digital surface models (DSMs) with 0.027 to 0.28 m resolution (we refer to these as DSMs rather than DEMs because vegetation is not removed from the DSMs) and orthomosaics of the 7 hillslope transects. We used the orthomosaics to identify and measure exposed beds on the hillslopes.

We identified inflection points in the landscape first using a map with a 10-meter DEM, where we visually determined places on hillslopes that appeared to be changing from generally high to low sloping areas and noticed that this appeared to be at approximately 16.7 to 21.8 degrees, ultimately adopting a value of 20 degrees as our marker due to the lower resolution of the DEM. We observed that at lower elevation areas, slope was higher, until it started decreasing at elevations which change for the different transects- we interpret these slope breaks to be inflection points where we can bin landscape sections into different categories. Subsequently, with a higher resolution 1-meter DEM, we examined curvature and slope along seven transects. We pinpointed locations with less noisy curvature as areas where the landscape became gentler and potentially relict. The transects exhibited a pattern of decreasing slope from higher to lower slopes, creating a transition zone where slope decreased slightly, typically below 20 degrees, before increasing again. Above this second inflection point, slope decreased steadily, indicating a diffuse section. For each transect, we identified two inflection points (arrows on figure 2): one where slope shifted from higher to intermediate values and another where slope decreased to a lower, more diffuse state.


Our study in Last Chance Canyon, has shown three conclusions that shape the landscapes geometry. Firstly, the variance in bed thickness has a profound impact on hillslope form, with thicker beds diminishing the signal of transience above them and possibly changing the direction of erosion into the hillslopes. Second, the hillslope's location within the landscape engenders distinct forms, with lower elevation hillslopes and hillslopes with greater drainage areas bearing the more pronounced imprint of the erosional wave resulting from base level fall. Lastly, the combined influence of these factors drives the intricate morphology of the hillslopes: Thick beds inhibit and redirect the erosional wave as it progresses upslope, and the presence of thin beds above these thick beds allow for the hillslopes to be shallow and diffuse. These conclusions underscore the intricate interplay between bed thickness, hillslope position relative to the erosional wave, and the erosional wave's direction of movement as governed by thick beds.



THIN BEDS ARMORED FROM BELOW ERODING BACK INTO HS. Stars on the map different then profile. Make the big beds symbology bigger. The presence of substantial beds significantly impacts the inflection points and hillslope morphology in Last Chance Canyon. Below the lower inflection point in all seven transects, the landscape features steep, high-gradient segments indicative of active adjustment in response to the erosional wave's upstream progression. At the first inflection point, the erosional wave encounters an obstruction, resulting in temporary stalling and some diffusion, while the landscape retains its steep and adjusting character below this point. In elevations higher than the lower inflection point but lower than the higher inflection point, the lingering influence of the erosional wave is observed, although diffused. Above the second inflection, higher elevation inflection point, the landscape exhibits lower slopes and is interpreted to be relict and reminiscent of the pre-base-level fall topography. The thickness of beds below the lower and upper inflection points significantly affects the elevation and angle between these inflection points. In LC3, the presence of an approximately 20-meter-thick bed near the base of the watershed obstructs the progress of the erosional wave, here, the wave's direction is altered, prompting it to erode into the hillslope and form a distinctive nick point in the landscape. Below this point, slopes are steep, while above it, slopes become shallower. In contrast, LC1 features relatively thick beds at similar elevations, leading to the development of gentler slopes at the inflection points.

Due to the substantial bed at the base of LC3, the erosional wave is effectively impeded and diffused as it ascends the slope. Consequently, the inflection points in LC3 are distributed at varying elevations. At the lowest downstream point of LC3, the inflection points are positioned at a lower elevation, approximately 1550 meters and the location of the 20m thick bed. In contrast, at the top of LC3, the lower inflection point is situated at a higher elevation, around 1660 meters. This configuration results in an angled landscape in LC3, the angle being dictated by the elevations of the lower inflection points. In contrast to LC3, LC1 presents a distinct scenario. LC1 lacks the presence of large, competent beds at its base, and as a result, the erosional wave has managed to propagate nearer to the ridgeline in all three of its transects. There is a 15.73 m bed at the very base of the most downstream transect in LC1, but its location speaks to it being recently exposed on the landscape and it’s signal has likely not yet been expressed on the landscape. It's also worth noting that the transects in LC1 are relatively closer together and at similar elevations when compared to the transects in LC3. This proximity indicates a similar history for the three transects, and the lack of large beds at the scale of the one in LC3 has allowed the erosional wave to travel upward, and the signal is consistently inhibited at approximately the same elevation for the three transects. This causes the inflection points to be at a similar elevation in LC1 with only a slight positive upslope trend which is interpreted to be a small signal from the erosional waves upslope direction of propagation.

What sets LC3 apart is the 1) presence of a very large bed near the base of the watershed, and 2) the longer length that the erosional wave has had to move across relative to LC1. The lower inflection points in LC3 create a relatively linear angle angled upwards in elevation, moving progressively from lower to higher elevations across the watershed. Conversely, the upper inflection points in LC3 exhibit a non-linear angle, curving and flattening as you move from upstream to downstream. This observation can be attributed to the presence of larger bed thicknesses in the lower elevation sections of LC3. In the downstream sections, these substantial beds act as obstacles, impeding the erosional wave and causing it to diffuse above them. As this diffused signal advances upslope, it does so at a different angle. It appears to move parallel to the large beds into the landscape situated just above them, particularly in the two downstream sections or transects of LC3. In contrast, in the upstream part of LC3, the beds are not as substantial, and the erosional wave, while diffused by the time it reaches them, propagates only a short distance upstream of the beds.

A diagram of a plane

Description automatically generated

There is a clear relationship between the thickness of the beds below the lower inflection point and the vertical distance between the lower and upper inflection points. When larger beds are present below the lower inflection point, the vertical separation between the upper and lower inflection points tends to be greater. This occurs because substantial beds are typically situated at lower elevations, causing the erosional wave to cross them and ascend until it eventually reaches and halts at the upper inflection point. If the lower beds are thinner, or non existent, then the elevation that the wave has propagated to will be higher or will have reached the ridgeline. Its important to note that all three transects in LC1 feature a series of substantial beds at approximately 1640 meters in elevation. These beds exhibit similar thicknesses, and they effectively obstruct the erosional signal, causing it to propagate upward to the higher inflection point at roughly the same distance for all three transects within LC1. Where LC3 the transects are spaced farther apart and the thickness of the beds below the lower inflection point are more variant, causing the distances between the upper and lower inflection points to be more disparate.

The bed thickness below the lower inflection point attenuates the erosional signal at elevations above it, leading to the lower inflection point being at a lower elevation. In contrast, the thickness of the bed below the upper inflection point alters the angle between the two inflection points. Thicker beds result in a larger angle, while thinner or absent beds lead to a smaller angle. The maximum angle observed in our study is 0.4 degrees. This change in angle is a consequence of the interaction between bed thickness and the erosional wave above the lower inflection point, where the wave has already been attenuated. As the erosional wave ascends, it encounters a substantial bed at a lower elevation. This interaction causes the wave's signal to change direction, become diminished, and ultimately cease at a bed just below the upper inflection point. The size of the bed below the upper inflection point affects the angle between the inflection points, resulting in a greater angle when a thicker bed is present. Where there are no measured beds below the upper inflection point, at 1654 m elevation at the farthest downstream transect in LC1 and one at 1613 m elevation in the second transect upstream in LC3, this represents the farthest the erosional wave has propagated before “petering out” of its own accord and with no input from a thick bed.

As the erosional wave advances from the base of the range towards its summit due to base level fall, it encounters these beds. When it encounters more resistant or competent beds, the wave diffuses, making the erosional signal less apparent at elevations beyond the reach of these competent, large, and thick beds.­­­­ Beyond the upper inflection point, the signal from the erosional wave dissipates. This outcome is influenced by the hillslope's location in the landscape and the extent to which the erosional wave has been able to ascend in elevation. The thickness of the beds it encounters plays a critical role in this process. In our specific landscape, thicker beds are generally found at lower elevations, contributing to steeper slopes in those areas due to adjustments resulting from base level fall. As the erosional wave advances, it climbs until it intersects the lower inflection point. At this juncture, the wave is attenuated and eventually ceases at the upper inflection point. The vertical distance between the upper and lower inflection points is greater when the erosional wave has not encountered substantial beds, as these beds reduce the impact and imprint of the erosional wave on hillslope form.

In the case of Last Chance Canyon, you can utilize the concept of space-for-time substitution by examining the inflection points where hillslope forms change. These inflection points indicate shifts in the landscape's characteristics, often associated with different phases in the landscape's development. By analyzing these inflection points along the canyon, one can gain insights into the canyon's evolutionary history. For example, if you observe that the lower inflection points in the canyon are characterized by steeper, higher-gradient slopes while the upper inflection points exhibit lower slopes and relict features, this suggests a spatial progression from a more actively adjusting and erosive landscape near the base of the canyon (younger stage) to a less dynamic, older landscape further upstream. In essence, these inflection points serve as markers in space that represent different phases in the canyon's development. By analyzing the spatial distribution and characteristics of these inflection points along the canyon, you can infer the temporal evolution of Last Chance Canyon, demonstrating how it has changed and matured over time.

In summary, our exploration of Last Chance Canyon's hillslope geometry has revealed three critical conclusions. Firstly, the variability in bed thickness significantly influences hillslope form and geometry. Second, the location of a hillslope within the landscape results in distinct forms, with those at lower elevations bearing a more pronounced imprint of the erosional wave stemming from base level fall. These two factors dynamically interact to shape hillslope morphology, with larger beds at lower elevations inhibiting and altering the direction of the erosional wave as it propagates upslope. This intricate relationship between bed thickness, hillslope position, and the erosional wave's behavior represents a fundamental driver of the observed hillslope morphology within the Last Chance Canyon landscape. Furthermore, an erosional wave progressing through a horizontally bedded landscape encounters challenges when reaching large beds, leading to a loss of intensity as it becomes 'stuck' downstream. Simultaneously, its intensity is influenced by the increase in alluvial material contributed by the hillslopes as it moves upstream. This presence of the erosional wave prompts the landscape to react by orienting the inflection point between relict and adjusting topography positively with diminishing drainage area and/or increasing distance upstream, impacting the natural curvature change across a hillslope. Lastly, our interpretation suggests that large beds diminish the erosional signal at higher elevations from base level fall. The diffuse hillslopes at the top of Last Chance Canyon have a base level that is pinned by the thick beds downslope of them. Together, these findings highlight the complex interplay of bed thickness, hillslope positioning, and the erosional wave in shaping hillslope morphology, providing valuable insights into the processes that drive hillslope dynamics within this unique landscape.

# Old References

Bell, F. G. (2005). ENGINEERING GEOLOGY| Problematic Rocks.

Bursztyn, N., Pederson, J. L., Tressler, C., Mackley, R. D., & Mitchell, K. J. (2015). Rock strength along a fluvial transect of the Colorado Plateau – quantifying a fundamental control on geomorphology. Earth and Planetary Science Letters, 429, 90–100. doi:10.1016/j.epsl.2015.07.042

Chapin, C. E., Cather, S. M., & Keller, G. R. (1994). Tectonic setting of the axial basins of the northern and central Rio Grande rift. Special Papers-Geological Society of America, 5–5.

Chilton, K. D., & Spotila, J. A. (2020). Preservation of Valley and Ridge topography via delivery of resistant, ridge-sourced boulders to hillslopes and channels, Southern Appalachian Mountains, U.S.A. Geomorphology, 365, 107263. doi:10.1016/j.geomorph.2020.107263

Darling, A., & Whipple, K. (08 2015). Geomorphic constraints on the age of the western Grand Canyon. Geosphere, 11(4), 958–976. doi:10.1130/GES01131.1

Decker, D. D., Polyak, V. J., Asmerom, Y., & Lachniet, M. S. (2018). U--Pb dating of cave spar: a new shallow crust landscape evolution tool. Tectonics, 37(1), 208–223.

DiBiase, R. A., Rossi, M. W., & Neely, A. B. (2018). Fracture density and grain size controls on the relief structure of bedrock landscapes. Geology, 46(5), 399–402. doi:10.1130/G40006.1

DiBiase, R. A., Whipple, K. X., Heimsath, A. M., & Ouimet, W. B. (2010). Landscape form and millennial erosion rates in the San Gabriel Mountains, CA. Earth and Planetary Science Letters, 289(1), 134–144. doi:10.1016/j.epsl.2009.10.03

Duvall, A., Kirby, E., & Burbank, D. (2004). Tectonic and lithologic controls on bedrock channel profiles and processes in coastal California. Journal of Geophysical Research: Earth Surface, 109(F3). doi:10.1029/2003JF000086

Forte, A. M., Yanites, B. J., & Whipple, K. X. (2016). Complexities of landscape evolution during incision through layered stratigraphy with contrasts in rock strength. Earth Surface Processes and Landforms, 41(12), 1736–1757. doi:10.1002/esp.3947 Finnegan, N. J., Klier, R. A., Johnstone, S., Pfeiffer, A. M., & Johnson, K. (2017). Field evidence for the control of grain size and sediment supply on steady-state bedrock river channel slopes in a tectonically active setting. Earth Surface Processes and Landforms, 42(14), 2338–2349.

Harel, M.-A., Mudd, S. M., & Attal, M. (2016). Global analysis of the stream power law parameters based on worldwide 10Be denudation rates. Geomorphology, 268, 184–196. doi:10.1016/j.geomorph.2016.05.035

Healy, D., Rizzo, R. E., Cornwell, D. G., Farrell, N. J. C., Watkins, H., Timms, N. E., … Smith, M. (2017). FracPaQ: A MATLABTM toolbox for the quantification of fracture patterns. Journal of Structural Geology, 95, 1–16.

Hill, C. A. (1987). Geology of Carlsbad cavern and other caves in the Guadalupe Mountains, New Mexico and Texas. Bull. 117, New Mexico Bureau of Mines and Minerals Resources.

Hill, C. A., & Others. (2000). Overview of the geologic history of cave development in the Guadalupe Mountains, New Mexico. Journal of Cave and Karst Studies, 62(2), 60–71.

Hill, C. A. (2006). Geology of the Guadalupe Mountains: An overview of recent ideas. Caves and karst of southeastern New Mexico: Guidebook, 57th Field Conference, New Mexico Geological Society, Guidebook, 57th Field Conference, 145–150.

Hilley, G. E., & Arrowsmith, J. R. (2008). Geomorphic response to uplift along the Dragon’s Back pressure ridge, Carrizo Plain, California. Geology, 36(5), 367–370.

Hoffman, L. L. (2014). Spatial variability of erosion patterns along the eastern margin of the Rio Grande Rift. Illinois State University.

Jansen, J. D., Codilean, A. T., Bishop, P., & Hoey, T. B. (2010). Scale dependence of lithological control on topography: Bedrock channel geometry and catchment morphometry in western Scotland. The Journal of geology, 118(3), 223–246.

Johnson, J. P. L., Whipple, K. X., Sklar, L. S., & Hanks, T. C. (2009). Transport slopes, sediment cover, and bedrock channel incision in the Henry Mountains, Utah. Journal of Geophysical Research: Earth Surface, 114(F2). doi:10.1029/2007JF000862

Katz, O., Reches, Z., & Roegiers, J.-C. (2000). Evaluation of mechanical rock properties using a Schmidt Hammer. International Journal of rock mechanics and mining sciences, 37(4), 723–728.

Keen-Zebert, A., Hudson, M. R., Shepherd, S. L., & Thaler, E. A. (2017). The effect of lithology on valley width, terrace distribution, and bedload provenance in a tectonically stable catchment with flat-lying stratigraphy. Earth Surface Processes and Landforms, 42(10), 1573–1587.

Kerans, C., Zahm, C., Garcia-Fresca, B., & Harris, P. M. (2017). Guadalupe Mountains, West Texas and New Mexico: Key excursions. AAPG Bulletin, 101(4), 465–474.

Kirby, E., & Whipple, K. X. (2012). Expression of active tectonics in erosional landscapes. Journal of structural geology, 44, 54–75.

Konare, A., Zakey, A. S., Solmon, F., Giorgi, F., Rauscher, S., Ibrah, S., & Bi, X. (2008). A regional climate modeling study of the effect of desert dust on the West African monsoon. Journal of Geophysical Research: Atmospheres, 113(D12).

Lai, L. S.-H., Roering, J. J., Finnegan, N. J., Dorsey, R. J., & Yen, J.-Y. (2021). Coarse sediment supply sets the slope of bedrock channels in rapidly uplifting terrain: Field and topographic evidence from eastern Taiwan. Earth Surface Processes and Landforms, 46(13), 2671–2689. doi:10.1002/esp.5200

Montgomery, D. R., & Gran, K. B. (2001). Downstream variations in the width of bedrock channels. Water Resources Research, 37(6), 1841–1846. doi:10.1029/2000WR900393

Murphy, B., Johnson, J., Gasparini, N., & Sklar, L. (04 2016). Chemical weathering as a mechanism for the climatic control of bedrock river incision. Nature, 532, 223–227. doi:10.1038/nature17449

National Park Service Resources Inventory Program Lakewood Colorado, (2007). Digital geologic map of Guadalupe Mountains National Park and vicinity, Texas (NPS, GRD, GRE, GUMO).

Niedzielski, T., Migoń, P., & Placek, A. (2009). A minimum sample size required from Schmidt hammer measurements. Earth Surface Processes and Landforms: The Journal of the British Geomorphological Research Group, 34(13), 1713–1725.

Perne, M., Covington, M. D., Thaler, E. A., & Myre, J. M. (2017). Steady state, erosional continuity, and the topography of landscapes developed in layered rocks. Earth Surface Dynamics, 5(1), 85–100. doi:10.5194/esurf-5-85-2017

Phelps, R. M., Kerans, C., Scott, S. Z., Janson, X., & Bellian, J. A. (2008). Three-dimensional modelling and sequence stratigraphy of a carbonate ramp-to-shelf transition, Permian Upper San Andres Formation. Sedimentology, 55(6), 1777–1813.

Ricketts, J. W., Karlstrom, K. E., Priewisch, A., Crossey, L. J., Polyak, V. J., & Asmerom, Y. (2014). Quaternary extension in the Rio Grande rift at elevated strain rates recorded in travertine deposits, central New Mexico. Lithosphere, 6(1), 3–16.

Scharf, T. E., Codilean, A. T., De Wit, M., Jansen, J. D., & Kubik, P. W. (2013). Strong rocks sustain ancient postorogenic topography in southern Africa. Geology, 41(3), 331–334.

Scholle, P. A., Ulmer, D. S., & Melim, L. A. (1992). Late-stage calcites in the Permian Capitan Formation and its equivalents, Delaware Basin margin, west Texas and New Mexico: evidence for replacement of precursor evaporites. Sedimentology, 39(2), 207–234.

Schwanghart, W., & Scherler, D. (2014). Short Communication: TopoToolbox 2 – MATLAB-based software for topographic analysis and modeling in Earth surface sciences. Earth Surface Dynamics, 2(1), 1–7. doi:10.5194/esurf-2-1-2014

Sklar, L. S., & Dietrich, W. E. (12 2001). Sediment and rock strength controls on river incision into bedrock. Geology, 29(12), 1087–1090. doi:10.1130/0091-7613(2001)029<1087:SARSCO>2.0.CO;2

Spotila, J. A., Moskey, K. A., & Prince, P. S. (2015). Geologic controls on bedrock channel width in large, slowly-eroding catchments: Case study of the New River in eastern North America. Geomorphology, 230, 51–63. doi:10.1016/j.geomorph.2014.11.004

Thaler, E. A., & Covington, M. D. (2016). The influence of sandstone caprock material on bedrock channel steepness within a tectonically passive setting: Buffalo National River Basin, Arkansas, USA. Journal of Geophysical Research: Earth Surface, 121(9), 1635–1650. doi:10.1002/2015JF003771

Tranel, L. M., & Happel, A. A. (2020). Evaluating escarpment evolution and bedrock erosion rates in the western Guadalupe Mountains, West Texas and New Mexico. Geomorphology, 368, 107335.

US Geologic Survey, 2017, 1/3rd arc-second digital elevation models (DEMs). USGS National Map 3DEP downloadable data collection.

Verdian, J. P., Sklar, L. S., Riebe, C. S., & Moore, J. R. (2021). Sediment size on talus slopes correlates with fracture spacing on bedrock cliffs: implications for predicting initial sediment size distributions on hillslopes. Earth Surface Dynamics, 9(4), 1073–1090.

Whipple, K. X., & Tucker, G. E. (1999). Dynamics of the stream-power river incision model: Implications for height limits of mountain ranges, landscape response timescales, and research needs. Journal of Geophysical Research: Solid Earth, 104(B8), 17661–17674. doi:10.1029/1999JB900120

Wobus, C., Whipple, K. X., Kirby, E., Snyder, N., Johnson, J., Spyropolou, K., … Sheehan, D. (01 2006). Tectonics from topography: Procedures, promise, and pitfalls. Tectonics, Climate, and Landscape Evolution. doi:10.1130/2006.2398(04)

Wohl, E. E., Greenbaum, N., Schick, A. P., & Baker, V. R. (1994). Controls on bedrock channel incision along nahal paran, Israel. Earth Surface Processes and Landforms, 19(1), 1–13. doi:10.1002/esp.3290190102

Yanites, B. J., Becker, J. K., Madritsch, H., Schnellmann, M., & Ehlers, T. A. (2017). Lithologic effects on landscape response to base level changes: a modeling study in the context of the Eastern Jura Mountains, Switzerland. Journal of Geophysical Research: Earth Surface, 122(11), 2196–2222.

Yanites, B. J. (2018). The dynamics of channel slope, width, and sediment in actively eroding bedrock river systems. Journal of Geophysical Research: Earth Surface, 123(7), 1504–1527.

Zaleski, E., Eaton, D. W., Milkereit, B., Roberts, B., Salisbury, M., & Petrie, L. (1997). Seismic reflections from subvertical diabase dikes in an Archean terrane. Geology, 25(8), 707–710.

# New References

Mudd, Simon & Furbish, David. (1625). Influence of chemical denudation on hillslope morphology. Geomorphology J. Geophys. Res. 109. 10.1029/2003JF000087.

Shobe, C. M., Tucker, G. E., and Anderson, R. S. (2016), Hillslope-derived blocks retard river incision, Geophys. Res. Lett., 43, 5070– 5078, doi:10.1002/2016GL069262.

Neely, A. B., DiBiase, R. A., Corbett, L. B., Bierman, P. R., & Caffee, M. W. (2019). Bedrock fracture density controls on hillslope erodibility in steep, rocky landscapes with patchy soil cover, southern California, USA. Earth and Planetary Science Letters, 522, 186-197.

Ben-Asher, M., Haviv, I., Roering, J. J., & Crouvi, O. (2019). The potential influence of dust flux and chemical weathering on hillslope morphology: Convex soil-mantled carbonate hillslopes in the Eastern Mediterranean. Geomorphology, 341, 203-215.

Gilbert, G. K. (1909). The convexity of hilltops. The Journal of Geology, 17(4), 344-350.

Culling, W. E. H. (1960). Analytical theory of erosion. The Journal of Geology, 68(3), 336-344.

Roering, J. J., Kirchner, J. W., & Dietrich, W. E. (1999). Evidence for nonlinear, diffusive sediment transport on hillslopes and implications for landscape morphology. Water Resources Research, 35(3), 853-870.

Tucker, G. E., & Bras, R. L. (1998). Hillslope processes, drainage density, and landscape morphology. Water resources research, 34(10), 2751-2764.

Mikey code https://github.com/mikafur32/PebbleCounts-Application-UI-and-Excel-Compiler/tree/main

https://pubs.geoscienceworld.org/gsa/geology/article/36/5/367/29716/Geomorphic-response-to-uplift-along-the-Dragon-s

4 figures, 3000 words (science), 18,500 characters (geology), referenced summary (200 words), 6 pages 2500 words (nature), 5 pages 3000 words (science)